----------------------------
Network stumbler flags
----------------------------
??1? - encrypted
??0? - unencrypted


----------------------------
Wifi range
----------------------------
A typical wireless router using 802.11b or 802.11g with a stock antenna might have a range of 32 m (120 ft) indoors and 95 m (300 ft) outdoors.
http://en.wikipedia.org/wiki/Wi-Fi

A general rule of thumb in home networking says that 802.11b and 802.11g WAPs and routers support a range of up to 150 feet (46 m) indoors and 300 feet (92 m) outdoors. 
http://compnetworking.about.com/cs/wirelessproducts/f/wifirange.htm


----------------------------
Gheat
----------------------------
Getest met 1.000, 10.000, 100.000 en 1.000.000 random punten. Werkt, maar meer punten zal langere rendertijd als gevolg hebben. Eenmaal gerenderd zijn de afbeeldingen instant op te roepen, laat server bijv snachts renderen zodat het geen probleem vormt.


----------------------------
Layers
----------------------------
Getest; 2 gheat-layers met een OLHeatmap layer erbj. Werkt, gaat wel ten koste van performance (al kan/zal dit ook liggen aan hoeveelheid data die OLHeatmap moet renderen).